**Release Notes:**

PSSE CDS case issue date: 27/06/2014

*Notes:*

* As agreed with the EA, the SO is required to submit PSSE files for NIPS and SIPS, light load and typical load, for the Industry to use.
* Having discussed with the EA it was decided to deliver a raw file for each version of PSSE since these files do not occupy too much space.
* These cases have been derived from the Power-Factory CDS (Central Data Set) files submitted earlier and have been checked against Power-Factory for accuracy.
* Since PSSE looks at Bus Numbers and not Bus names a number has been assigned to each Bus in PSSE. These Bus Numbers will be consistent for every PSSE release in the future with new Bus Numbers being added whenever there is a new bus commissioned on the grid. This is for the ease of use of the Industry participants who might have drawings based on these Bus Numbers.

*Files submitted in the format:* (North Island/South Island­\_typical load case/light load case\_PSSE versions.raw)

SI\_typical\_15\_23.raw - (South Island typical case for PSSE versions 15 till 23)

SI\_typical\_24\_26.raw - (South Island typical case for PSSE versions 24 till 26)

SI\_typical\_27\_28.raw - (South Island typical case for PSSE versions 27 till 28)

SI\_typical\_29.raw - (South Island typical case for PSSE version 29)

SI\_typical\_30.raw - (South Island typical case for PSSE version 30)

SI\_typical\_31.raw - (South Island typical case for PSSE version 31)

SI\_typical\_32.raw - (South Island typical case for PSSE version 32)

SI\_light\_15\_23.raw - (South Island light case for PSSE versions 15 till 23)

SI\_ light \_24\_26.raw - (South Island light case for PSSE versions 24 till 26)

SI\_ light \_27\_28.raw - (South Island light case for PSSE versions 27 till 28)

SI\_ light \_29.raw - (South Island light case for PSSE versions 29)

SI\_ light \_30.raw - (South Island light case for PSSE versions 30)

SI\_ light \_31.raw - (South Island light case for PSSE versions 31)

SI\_ light \_32.raw - (South Island light case for PSSE versions 32)

NI\_typical\_15\_23.raw - (North Island typical case for PSSE versions 15 till 23)

NI\_typical\_24\_26.raw - (North Island typical case for PSSE versions 24 till 26)

NI\_typical\_27\_28.raw - (North Island typical case for PSSE versions 27 till 28)

NI\_typical\_29.raw - (North Island typical case for PSSE versions 29)

NI\_typical\_30.raw - (North Island typical case for PSSE versions 30)

NI\_typical\_31.raw - (North Island typical case for PSSE versions 31)

NI\_32.raw - (North Island typical case for PSSE versions 32)

NI\_light\_15\_23.raw - (North Island light case for PSSE versions 15 till 23)

NI\_ light \_24\_26.raw - (North Island light case for PSSE versions 24 till 26)

NI\_ light \_27\_28.raw - (North Island light case for PSSE versions 27 till 28)

NI\_ light \_29.raw - (North Island light case for PSSE versions 29)

NI\_ light \_30.raw - (North Island light case for PSSE versions 30)

NI\_ light \_31.raw - (North Island light case for PSSE versions 31)

NI\_ light \_32.raw - (North Island light case for PSSE versions 32)